**Copper tails**

M10 x 1 L. 363mm

2 pieces

Reference: **811612.2P**

Specification description

Soft-tempered copper tails M10 X 1 L. 363mm to supply mixers.

Can be installed instead of PEX flexibles.

Improves efficiency of thermal shocks.

Supplied in packs of 2.

Pro tip: Don't forget to include non-return valves on the copper tails if the PEX flexibles to be replaced have integral non-return valves. Call our Technical Team for more information.