**AZA Urinal divider**

Polished satin 304 stainless steel - H. 600mm

Reference: **100620**

Specification description

Urinal divider for wall-mounting.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 3mm.

Smooth surface and rounded edges.

Supplied with fixing elements and TORX anti-theft screws.

Weight: 4kg.