**Recessed waterproof housing for BINOPTIC**

Mains supply, kit 1/2

Recessed, waterproof

Reference: **370SBOX**

Specification description

Recessed waterproof housing for BINOPTIC 2, kit 1/2:

Mains supply 230/6V (cable and transformer supplied).

Recessed waterproof housing:

- Collar with waterproof seal.

- Hydraulic connection from the exterior and maintenance from the front.

- Modular installation (rails, solid walls, panels).

- Compatible with walls from 10 to 120mm (whilst maintaining the minimum recessing depth of 83mm).

- Adaptable standard pipework or "pipe in pipe".

- Integrated stopcock and flow rate adjuster, filter and solenoid valve are accessible from the front.

- BINOPTIC 2 tap F½".

- Supplied in 2 kits: secured system purge without sensitive elements.

30-year warranty.

Order with control plate references: 370100 or 370110.