**TEMPOMIX 3 time flow basin mixer**

Soft-touch operation, kit 2/2

Single control, Recessed with spout L. 190mm

Reference: **794200**

Specification description

Recessed TEMPOMIX 3 basin mixer kit 2/2:

Tamperproof chrome-plated metal plate 160 x 160mm.

Temperature control and operation via the push-button.

Maximum temperature limiter (can be adjusted by installer).

Soft-touch operation.

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar pressure, can be adjusted 1.4 - 6 lpm.

Scale-resistant flow straightener.

Spout L. 110mm with smooth interior and low water volume (reduces niches where bacteria can develop).

Suitable for people with reduced mobility.

30-year warranty.

Order with 794BOX3 waterproof housing.