**SECURITHERM electronic shower kit**

Thermostatic electronic, kit 2/2

Recessed waterproof housing

Reference: **792459**

Specification description

Recessed thermostatic electronic shower, kit 2/2:

Tamperproof polished satin stainless steel control plate 195 x 220mm.

SECURITHERM thermostatic shower mixer ¾".

Anti-scalding failsafe: automatic shut-off if cold water fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Adjustable temperature from 32° to 40°C, pre-set at 38°C.

Battery-operated with CR-P2 223 6V Lithium battery.

Infrared presence detection. Shower starts when hand is 4cm from the sensor.

Shuts off voluntarily or automatically after ~60 seconds.

Duty flush (~60 seconds every 24 hours after the last use).

Flow rate set at 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant ROUND shower head with automatic flow rate regulation.

Concealed fixings, M½" stopcocks.

Integrated non-return valves and filters.

Chrome-plated Bayblend® control knob.

Electronic shower kit suitable for people with reduced mobility.

30-year warranty.

Order with recessed waterproof housing ref. 792BOX.