**Electronic SECURITHERM shower mixer**

Thermostatic electronic, kit 2/2

Recessed

Reference: **792452**

Specification description

Recessed thermostatic electronic shower mixer, kit 2/2:

Tamperproof satin stainless steel control plate 195 x 220mm.

SECURITHERM thermostatic shower mixer ¾".

Anti-scalding safety: automatic shut-off in the event of cold water failure.

Anti-cold showers function: automatic shut-off if hot water fails.

Adjustable temperature from 32° to 40°C, pre-set at 38°C.

Battery-operated with CR-P2 223 6V Lithium battery.

Infrared presence detection. Shower starts when hand is 4cm from the sensor.

Voluntary or automatic shut-off after ~60 seconds.

Duty flush (~60 seconds every 24 hours after last use).

Flow rate 9 lpm at 3 bar.

Concealed fixings, M½" stopcocks.

Integrated non-return valves and filters.

Chrome-plated Bayblend® control knob.

Electronic shower mixer suitable for people with reduced mobility`.

30-year warranty.

Order with waterproof housing ref. 792BOX.