**RAINY shower head**

Rain-effect shower head for panels

For panels 15mm maximum, Scale-resistant

Reference: **708010**

Specification description

Fixed shower head.

Flow rate 6 lpm at 3 bar.

A higher flow rate can be achieved: remove flow rate regulator.

Scale-resistant head with nozzles, ligature-resistant.

Soft rain-effect flow engulfs user.

Chrome-plated metal.

Easy installation system: install the connection in the wall and then clip the shower head to it.

Inlet M½".

Shower head for panels 15mm thick maximum.

30-year warranty.