**TEMPOFIX 3 frame system for urinals**

Steel frame system for urinals Ø 35mm

For wall-mounted installation

Reference: **543006**

Specification description

Frame system for urinals Ø 35mm, kit 1/2:

Black powder-coated steel frame for wall-mounted installation.

Fixes to floor and load-bearing walls with anchoring bolts supplied.

Adjustable bracket from 95 - 280mm.

Frame height can be adjusted from 0 to 200mm.

Ø 50mm soil pipe with waterproof seal and tube with connection washer Ø 35mm.

Delivered pre-mounted.

Compatible with solid wall finishes from 13 to 120mm.

Supplied with recessed housing

Valve configured for system flush, with accessories and connection protection.

30-year warranty.

Order with control plate references 430006, 430016, 430026,430036, 778700 or 778707.