**TEMPOFIX 3 frame system for urinals**

Steel frame system for urinal with flexible, 1/2"

For wall-mounted installation

Reference: **543000D**

Specification description

Steel frame system for urinal with flexible ½", kit ½:

Black powder-coated steel frame for wall-mounted installation.

Fixes to floor and load-bearing walls with anchoring bolts supplied.

Adjustable bracket from 95 - 280mm.

Frame height can be adjusted from 0 to 200mm.

Ø 50mm soil pipe with waterproof seal.

Tube with ½" brass connection for urinals with flexible inlet.

Delivered pre-mounted.

Compatible with solid wall finishes from 13 - 120mm.

Supplied with recessed housing.

Valve configured for system flush, with accessories and connection protection..

30-year warranty.

Order with control plate references 430000, 430010, 430020 or 430030.