**Single hole deck-mounted mixer**

Mechanical mixer - flexible has no retainer

Reference: **2526T2**

Specification description

Single hole deck-mounted mixer, flexible has no retainer, flexible H. 535mm maximum.

Mechanical mixer with flexible swivelling hand spray with smooth interior.

Optimised spout curve for easy access to the control lever: 379mm.

Ø 35mm ceramic cartridge.

Flow rate 9 lpm at 3 bar.

Slimline control lever.

Chrome-plated brass body.

PEX flexibles F3/8" with filters and non-return valves.

Reinforced fixings.

Mixer suitable for intensive use in professional kitchens.

Mixer with 30-year warranty.