**BIOSAFE hygienic outlet M16.5/100**

1 piece

Reference: **922660**

Specification description

BIOSAFE hygienic free flow outlet M16.5/100 for product ranges 2920 and 2664/2665.

No grid or partitions in contact with water.

Flow rate 5 lpm.

Water cannot stagnate in internal parts, reducing bacterial development.

Made from Hostaform®; reduces scale build-up.

Supplied individually.

For installation only on a mixer or tap with a restricted flow rate to ensure a laminar flow with no splashing.