**AQUEDUTO wall-mounted washbasin**

Matte black 304 stainless steel - Concealed drainage

Reference: **121150BK**

Specification description

Wall-mounted washbasin, 700 x 440mm

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 1.2mm.

Matte black Teflon® finish.

Rounded edges prevent injury.

With Ø 35mm central tap hole.

Supplied with 1¼" waste.

Without overflow.

Supplied with brackets and fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 12kg.

30-year warranty.