**Electronic control unit**

For TEMPOMATIC 4 urinals

Battery-operated

Reference: **479436**

Specification description

Electronic control unit.

For TEMPOMATIC 4 urinals.

Power supplied by 6V batteries.

Dimensions: 53 x 45mm, Ø 51mm.