**Detector**

For TEMPOMATIC

L.1.45m cable

Reference: **495149**

Specification description

Detector.

For TEMPOMATIC basin, shower, urinal and WC.

With 1.45m cable.