**TEMPOMIX time flow basin mixer**

Time flow single control

For panels 8 to 16mm

Reference: **790975**

Specification description

Exposed time flow basin panel:

TEMPOMIX ¾" single control mixer.

For panels from 8 to 16mm.

Temperature adjustment and operation on control.

Maximum temperature limiter (can be adjusted by installer).

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 12 lpm at 3 bar, can be adjusted.

Chrome-plated solid brass.

Integrated filters and non-return valves.

Chrome-plated metal control.

30-year warranty.