**BINOPTIC deck-mounted electronic soap dispenser**

Liquid soap, foam soap or hydroalcoholic gel dispenser

Mains, satin finish 304 stainless steel, 0.5L tank

Reference: **512521S**

Specification description

Deck-mounted electronic soap dispenser.

Liquid soap, foam soap or hydroalcoholic gel dispenser.

No manual contact: hands are automatically detected by infrared cell.

Spout made from satin finish 304 stainless steel.

No waste pump dispenser.

Separate electronic unit and removable tank for installation under the basin.

Automatic soap dispenser: mains supply with 230/6V transformer.

For vegetable-based liquid soap with a maximum viscosity of 3,000 mPa.s or specialist foam soap.

Compatible with hydroalcoholic gel.

Spout length: 105mm.

Supplied with a 0.5 litre tank.

BINOPTIC electronic soap dispenser with 30-year warranty.

CE marked.