**BINOPTIC deck-mounted electronic soap dispenser**

Liquid or foam soap dispenser

Mains, satin 304 stainless steel, with 1.2m tube

Reference: **512121S**

Specification description

Deck-mounted electronic soap dispenser.

Liquid or foam soap dispenser.

No manual contact: infrared cell detects hands automatically.

Satin finish 304 stainless steel spout.

No waste pump dispenser.

Separate electronic unit for installation beneath the washbasin.

Automatic soap dispenser: mains supply with 230/6V transformer.

For vegetable-based liquid soap with maximum viscosity of 3,000 mPa.s or specific foam soap.

Total spout length: 105mm.

Supplied with 1.20m flexible tube for remote tanks (tank not supplied).

Wall-mounted electronic soap dispenser with 30-year warranty.

CE marked.