**Thermostatic mixing valve repair kit**

For PREMIX COMFORT thermostatic mixing valve

For mixed water distribution from 32 to 42°C

Reference: **753735**

Specification description

Repair kit for the PREMIX COMFORT thermostatic mixing valve, after June 2008.

Cartridge with thermostatic cell.

Anti-scalding safety: shuts off automatically if the cold or hot water supply fails.

For PREMIX COMFORT 1"1/4 and 1"1/2.