**Be-Line® ambulant WC pack**

DOC M pack

Metallised anthracite powder-coated aluminium

Reference: **511811MC**

Specification description

DOC M Be-Line® WC pack with 3 grab bars, length 600mm.

Aluminium tube Ø 35mm.

Metallised anthracite powder-coated finish (LRV 14) provides a good visual contrast with the wall.

Tested to over 200kg.

Maximum recommended user weight 135kg.

30-year warranty.

CE marked.

DOC M compliant.