**PREMIX COMPACT Thermostatic mixing valve**

For mixed water 30 - 60 °C

Nickel-plated brass body, 1 to 11 outlets, Ø 15mm

Reference: **733115**

Specification description

Thermostatic mixing valve for mixed water distribution from 30 - 60°C.

To supply 1 to 11 points-of-use (depending on the flow rate).

Anti-scalding safety: shuts off automatically if the cold or hot water supply fails.

Temperature can be adjusted from 30 - 60 °C, can be locked by the installer.

Brass body.

Filters and non-return valves.

Recommended flow rate range: from 5 - 33 lpm.

Thermal shocks are possible.

M1/2" Ø 15mm.

Centres: 40mm.

30-year warranty.