**Be-Line® shower stool**

White seat

304 stainless steel structure

Reference: **511418W**

Specification description

Be-Line® shower stool

Stool for disabled people and people with reduced mobility.

Wide model with ergonomic handles.

Suitable for intensive use in public places and hospitals.

Solid white seat made from high strength polymer.

Non-slip surface.

Good resistance to Betadine®.

304 stainless steel structure Ø 18 x 2mm.

Anti-bacterial treatment: optimum protection against bacterial development.

Dimensions: 360 x 540 x 480mm.

Seat height: 480mm.

Tested to over 200kg. Maximum recommended user weight: 135kg.

Black plastic protective caps on feet.

Shower stool with 30-year warranty.