**Recessed nanny joint for SPORTING 2 SECURITHERM**

For SPORTING 2 SECURITHERM mains supply - Kit 1/2

Compact, for top or bottom supply inlet

Reference: **714012**

Specification description

Recessed nanny joint, kit 1/2:

Compact nanny bracket for SPORTING 2 SECURITHERM mains supply shower panels.

Recessed top or bottom inlet.

Delivered with buttons pre-mounted for pressure test.

Fixing plate is easy to install: bayonette system to allow maintenance of the caps in situ.

Mounted with screwdriver or pliers.

Modular installation (plaster rails, solid walls):

- Installation with plaster rails (with or without struts): compatible with panels between 24 and 68mm (with a minimum recessing depth of 48mm).

- Installation with solid walls: compatible with panels between 0 and 68mm.

Secured system purge without sensitive elements.

Connector M1/2".

30 year warranty.

Order with recessed mains supply SPORTING 2 SECURITHERM shower panel reference 714910.