**Wall-mounted CANAL wash trough**

Polished satin 304 stainless steel - L. 1800mm

Without tap hole - drainage on the left

Reference: **122280**

Specification description

Wall-mounted wash trough, 3 - 4 services - 1800mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 0.8mm for the bowl, 1.5mm for surround and fixing brackets.

Easy to install: no joint concealers to install, lightweight trough.

Water control can be wall-mounted or deck-mounted.

Drainage on the left.

Without tap hole.

Supplied with 1¼" waste. Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14296.

Weight: 10.3kg.

Possible to add a bacteriostatic 304 stainless steel splashback (ref. 100280).

30-year warranty.