**Hygienic waste without water level**

Waste without water level, with membrane

Chrome-plated waste

Reference: **621**

Specification description

Water-free waste M1 1/4".

Waste with a membrane to prevent bad smells.

No water level: cap and cup with a membrane which can be removed from above.

Membrane can be cleaned and replaced.

Cap made from stainless steel. Cup and body made from polypropylene. Membrane made from silicone.

Evacuation flow rate complies with European standard EN 274: 36 lpm.

Waste can be cut to size.

Not suitable for washbasins with an overflow.

30-year warranty.