**Wall-mounted sequential mechanical basin mixer**

Sequential mechanical mixer with swivelling spout

With STOP/CHECK connectors

Reference: **2436**

Specification description

Wall-mounted sequential mechanical basin mixer.

Sequential over 90°: opens and closes with cold water.

Flat swivelling under-spout, L. 200mm, with hygienic flow straightener suitable for fitting a BIOFIL point-of-use filter.

Securitouch thermal insulation prevents burns.

Ø 35mm ceramic cartridge.

Pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume. (reduces bacterial development).

Flow rate regulated at 5 lpm.

Hygiene lever L. 150mm.

Supplied with 2 wall-mounted STOP/CHECK connectors, M1/2" M3/4".

Suitable for people with reduced mobility.

30-year warranty.