**TEMPOSTOP 3 time flow shower valve**

Time flow

Exposed, in-line, M1/2"

Reference: **703500**

Specification description

Exposed time flow shower valve:

TEMPOSTOP 3 M1/2" time flow valve; supply with mixed water.

Wall-mounted exposed installation.

In-line model for in-line supply.

~30 seconds time flow.

Flow rate pre-set at 9 lpm at 3 bar, can be adjusted.

Chrome-plated brass body.

Chrome-plated metal push-button.

30-year warranty.