**RAVA black countertop washbasin**

Matte black 304 stainless steel - Countertop

Reference: **120670BK**

Specification description

Round countertop washbasin, semi-recessed, 420 x 420mm.

Suitable for classic or tall taps and wall-mounted mixers.

Basin internal diameter: 385mm.

Cut-out diameter: 385mm.

Bacteriostatic 304 stainless steel.

Matte black Teflon® finish.

Stainless steel thickness: 1mm.

One-piece, seam-free pressed bowl.

Rounded edges prevent injury.

Supplied without waste. Option to add a waste with a black finish (6110BK) or a chrome-plated finish (6110).

Without overflow.

CE marked. Complies with European standard EN 14688.

Weight: 2.6kg.

30-year warranty.