20804T2

**TEMPOMATIC electronic tap for sinks with BIOCLIP removable spout**

Reference: 20804T2

Specification Description

Wall-mounted electronic tap with BIOCLIP spout, for mounting on panels &lt; 20mm.

Independent IP65 electronic control unit.

Mains supply via 230/12V transformer.

Flow rate limited to 5 lpm at 3 bar.

Comes with 2 removable stainless steel spouts L. 188mm Ø 28mm.

Base and spout with smooth interior (reduces niches where bacteria can develop).

Adjustable duty flush (pre-set to approx. 60 secs every 24h after last use) in order to prevent water stagnation in the network in the event of prolonged periods of non-use.

Separate sensor for mounting on panels.

 M3/8" solenoid valve with integrated filter.

Shock-resistant infrared presence detection sensor.

Chrome-plated Ø 60mm brass base.

Anti-blocking security.

Recommended installation height: 110-200mm above the basin surface.

Two shut-off options:

- standard mode: timed flow with automatic shut-off.

- ON/OFF mode: user shuts off flow voluntarily after 30 minutes.

 Thermal shocks are possible.

10-year warranty.