2211LEP

**Pressure-balancing mixer with retracting hand spray**

Reference: 2211LEP

Specification Description

SECURITHERM pressure-balancing sink mixer with swivelling spout L. 200mm H. 105mm.

Ideal for babies' baths.

Anti-scalding safety: HW flow rate is reduced if CW supply fails.

Securitouch thermal insulation prevents burns.

Retracting hand spray with 2 jet options: flow straightener / rain effect.

Ø 40mm pressure-balancing ceramic cartridge with pre-set maximum temperature limiter.

Body with smooth interior.

Flow rate 12 lpm at 3 bar.

Mixed water brass outlet L. 105mm.

BIOSAFE flexible shower hose reduces bacterial proliferation: transparent polyurethane flexible hose, smooth interior and exterior, low water volume (interior Ø 6mm).

Specific counterweight.

Chrome-plated brass body and Hygiene control lever.

F⅜" PEX flexibles with filters and non-return valves.

Reinforced fixing via 2 stainless steel rods.

10-year warranty.