DELABIE_C100M352445LS

**Mechanical basin mixer**

Reference: 2445LS

Specification Description

Wall-mounted mechanical basin mixer.

Flat, swivelling under spout L. 200mm with hygienic flow straightener suitable for fitting a BIOFIL terminal filter.

Securitouch thermal insulation prevents burns.

Ø 40mm ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume (reduces bacterial niches).

Flow rate 5 lpm at 3 bar.

Chrome-plated brass body.

Hygiene control lever L. 150mm.

Supplied with standard connectors M1/2" M3/4".

10-year warranty.