2446EP

**SECURITHERM EP pressure-balancing basin mixer**

Reference: 2446EP

Specification Description

Wall-mounted SECURITHERM Pressure Balancing (EP) basin mixer.

Anti-scalding safety: HW flow is reduced if CW supply fails (and vice versa).

Securitouch thermal insulation prevents burns.

Flat, swivelling under spout L. 150mm with hygienic flow straightener suitable for fitting a BIOFIL terminal filter.

Ø 40mm pressure-balancing ceramic cartridge and pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume (reduces niches where bacteria can develop).

Flow rate regulated at 5 lpm.

Body and spout with smooth interior and low water volume (reduces bacterial development).

Chrome-plated brass body.

Sculptured control lever.

Supplied with STOP/CHECK connectors M1/2" M3/4" ideal for use in hospitals.

10-year warranty.