DELABIE_C100M352522L

**Mechanical basin mixer**

Reference: 2522L

Specification Description

Mechanical basin mixer with swivelling spout H. 95mm L. 170mm with hygienic flow straightener.

Ø 40mm ceramic cartridge.

Pre-set maximum temperature limiter.

Body and spout with smooth interiors.

Flow rate limited to 5 lpm at 3 bar.

Hygiene control lever L. 200mm.

Supplied with PEX flexibles F3/8".

Reinforced fixing via 2 stainless steel rods.