2564T4

**Mechanical mixer for sinks or troughs**

Reference: 2564T4

Specification Description

Mechanical mixer for sinks and troughs with swivelling spout H. 300mm L. 250mm.

High spout with hygienic flow straightener suitable for fitting a BIOFIL terminal filter.

Ø 40mm Ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors (reduced bacterial development).

Chrome-plated body, base and spout.

Flow rate limited to 9 lpm at 3 bar.

Hygiene control lever L. 215mm requires no manual contact.

Supplied with braided stainless steel PEX flexibles F3/8".

Reinforced fixings by 2 stainless steel rods and back-nuts.

10-year warranty.