28201TEP

**SECURITHERM EP BIOCLIP pressure-balancing basin mixer**

Reference: 28201TEP

Specification Description

SECURITHERM EP BIOCLIP pressure-balancing basin mixer H. 85mm L. 120mm with hygienic flow straightener.

Can be removed entirely for cleaning/disinfection.

Anti-scalding safety: HW flow rate is reduced if cold water supply fails (and vice versa).

Straight spout with hygienic flow straightener.

Ø 40mm ceramic cartridge with pressure-balancing.

Pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume (reduced bacterial development).

Flow rate limited to 5 lpm at 3 bar.

Solid control lever.

Ergonomic, brass pop-up waste 1 1/4".

Supplied with F3/8" PEX stainless steel braided flexibles with filters and non-return valves.

Reinforced fixing via 2 stainless steel rods.

10-year warranty,