35082S

**Basic angled grab bar 135°, satin, 400 x 400mm**

Reference: 35082S

Specification Description

Basic angled grab bar 135°, Ø 32mm, for people with reduced mobility.

Polished satin 304 stainless steel tube.

3 fixing points prevent the hand from getting trapped and simplify installation.

Dimensions: 400 x 400mm.

Concealed fixings secured to wall by 3-hole stainless steel plate.

CE marked.

10-year warranty.