DELABIE_C100M355086P2

**Angled grab bar 135°, Ø 25mm, 400 x 400mm**

Reference: 5086P2

Specification Description

Angled grab bar 135° for people with reduced mobility, Ø 25mm.

For use as a handrail (horizontal part) or as a grab bar (135° part) for WCs, showers or baths.

Universal for either left or right side.

Dimensions: 400 x 400mm.

Bacteriostatic 304 stainless steel tube.

Stainless steel with UltraPolish bright polished finish, non-porous uniform surface for easy maintenance and hygiene.

Plate welded to the tube by invisible bead weld (process exclusive to ArN-Securit).

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings, secured to wall by a 3-hole, 304 stainless steel plate, Ø 72mm.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight: 135kg.