DELABIE_C100M35511944W

**Be-line T-shaped shower grab bar with sliding vertical bar**

Reference: 511944W

Specification Description

Be-line T-shaped grab bar Ø 35mm for showers with sliding vertical bar..

Use as a shower rail and to support the user in an upright position.

Helps and secures entry and movement in the shower.

Use as a shower rail by adding a sliding shower head holder and/or soap dish.

Upright position can be adjusted during installation: can be moved to the left or the right in order to adapt the space

(positioning of shower, depth of shower seat...).

Dimensions: 1,130 x 500mm.

Aluminium tube thickness 3mm. Solid aluminium fixing points.

Rounded profile Ø 35mm with ergonomic flat front face that prevents rotation for an optimal grip.

Matte white powder-coated aluminium provides a good visual contrast with the wall.

Uniform surface for easy maintenance and hygiene.

38mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings.

Supplied with Ø 8 x 70 mm stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight: 135kg.

10-year warranty. CE marked.