512066P

**Wall-mounted electronic liquid soap dispenser, 1 litre**

Reference: 512066P

Specification Description

Electronic liquid soap dispenser, wall-mounted.

Vandal-resistant model with lock and standard DELABIE key.

No manual contact: hands are automatically detected by infrared cell (detection distance

can be adjusted).

Bacteriostatic 304 stainless steel cover.

One-piece hinged cover for easy maintenance

and better hygiene.

No waste pump dispenser: dispenses 0.8ml

(can be adjusted up to 7 doses per activation).

Option of operation in anti-clogging mode.

Power supply: 6 AA -1.5V (DC9V) batteries supplied integrated in the soap dispenser body.

Low battery indicator light.

Tank with large opening: eases transfer of soap

from large containers.

Window allows soap level to be checked.

Bright polished 304 stainless steel.

Stainless steel thickness: 1mm.

Capacity: 1 litre.

Dimensions : 90 x 105 x 256mm.

For vegetable-based liquid soap with a maximum viscosity of 3,000 mPa.s.

Compatible with hydroalcoholic gel.

CE marked.

10-year warranty.