H96051

**SECURITHERM BIOCLIP thermostatic basin mixer**

Reference: H96051

Specification Description

Deck-mounted thermostatic sequential SECURITHERM BIOCLIP basin mixer H. 85mm L. 120mm, without pop-up waste.

Removable mixer for easy cleaning/disinfection.

Anti-scalding failsafe: hot water shuts off immediately if cold water supply fails.

Securitouch thermal insulation prevents burns.

No non-return valves on the inlets.

Straight spout with hygienic flow straightener for no impurity retention and thermal shock-resistant.

Scale-resistant thermostatic sequential cartridge for single control of flow rate and temperature.

Cold water temperature adjustable up to 40°C with temperature limiter set at 40°C and thermal and chemical shocks are possible.

Body and spout with smooth interiors and low water volume.

Flow rate regulated at 7 lpm.

No manual contact thanks to Hygiene control lever L. 146mm.

Supplied with braided stainless steel flexibles made from PEX F3/8".

Reinforced fixing via 2 stainless steel rods.

10-year warranty.

Also available with copper tubes.