**Basic T-shaped white grab bar**

White powder-coated stainless steel

Ø 32mm

Reference: **35440W**

Specification description

Basic T-shaped shower grab bar for people with reduced mobility, Ø 32mm.

White powder-coated stainless steel tube.

Dimensions: 1,150 x 500mm.

Concealed fixings, secured to wall by a 3-hole stainless steel plate.

CE marked.

30-year warranty.