**Basic drop-down grab bar, white, L. 760mm**

White powder-coated stainless steel

Ø 32mm, visible fixings

Reference: **511516W**

Specification description

Basic drop-down grab bar Ø 32mm, for people with reduced mobility.

Drop-down grab bar made from white powder-coated stainless steel for WCs or showers.

Visible fixings, secured to wall by a 6-hole stainless steel plate.

Wall plate thickness: 3.5mm.

Dimensions: 760 x 300 x 100mm.

30-year warranty.

CE marked.

DOC M compliant.