**HOSPITAL bed pan cleaner with inverted hand spray**

With removable nozzle at a 30° angle

Reference: **15846**

Specification description

HOSPITAL bed pan cleaner with inverted hand spray and removable nozzle at a 30° angle: water flows when trigger is released (shut off the stopcock after use to avoid the flexible remaining under constant pressure).

Powerful jet for cleaning bed pans thoroughly with reduced risk of splashing.

Chrome-plated brass and white polypropylene.

Supplied with white, wall-mounted hook with screw.