**Flush tube**

For WC pan with TEMPOCHASSE 1"1/4

PE

Reference: **769001**

Specification description

Flush tube for WC:

For exposed TEMPOCHASSE.

Elbow flush tube Ø 32mm with nut 1 1/4".

Collar and connection washer Ø 32/55mm with clamp.

PE L. 215mm, H. 665mm.

30-year warranty.