**UNITO countertop washbasin**

Polished satin 304 stainless steel - Countertop

Without tap hole

Reference: **120810**

Specification description

Countertop washbasin, 395x350mm.

Suitable for use with wall-mounted or extended mixer/tap.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

Without tap hole.

Supplied with 1¼" waste.

Without overflow.

CE marked. Complies with European standard EN 14688.

Weight: 3.3kg.

30-year warranty.