**Towel rail**

Ø 20mm, 1 rail

304 white powder-coated stainless steel

Reference: **510788W**

Specification description

Towel rail for bathrooms.

Designer towel rail.

Robust model.

Rail Ø 20mm, length 600mm.

White powder-coated bacteriostatic 304 stainless steel.

Wall-mounted towel rail with concealed fixings.

30-year warranty.