**Surgical scrub-up trough with high upstand**

Polished satin 304 stainless steel - 1 service - "Hygiene+" Design

With twin tap holes Ø 22mm, c-c 150mm

Reference: **185200**

Specification description

Wall-mounted surgical scrub-up trough with 450mm upstand.

Suitable for hospitals and healthcare facilities.

Bacteriostatic 304 stainless steel. Polished satin finish. Stainless steel thickness: 1.2mm.

Length 700mm, 1 service. With twin tap holes Ø 22mm with 150mm centres.

Smooth surface and rounded inside edges for easy cleaning.

"Hygiene+" design: reduces niches where bacteria can develop.

Drainage on the right. Without overflow. Supplied with fixing elements.

CE marked. Complies with norm EN 14296.

Weight: 20.3kg

30-year warranty.