**BINOPTIC deck-mounted electronic soap dispenser**

Liquid soap, foam soap or hydroalcoholic gel soap dispenser

Mains, chrome-plated 304 stainless steel, 1L tank

Reference: **512021P**

Specification description

Deck-mounted electronic soap dispenser.

Liquid soap, foam soap or hydroalcoholic gel dispenser.

No manual contact: hands are automatically detected by infrared cell.

Spout made from chrome-plated 304 stainless steel.

No waste pump dispenser.

Separate electronic unit and removable tank for installation under the basin.

Automatic soap dispenser: mains supply with 230/6V transformer.

For vegetable-based liquid soap with a maximum viscosity of 3,000 mPa.s or specialist foam soap.

Compatible with hydroalcoholic gel.

Spout length: 105mm.

Supplied with a 1 litre tank.

30-year warranty.

CE marked.