**U-shaped toilet roll holder with spindle**

Toilet roll holder

Reference: **4081N**

Specification description

Wall-mounted U-shaped toilet roll holder.

Toilet roll holder.

White, high strength polyamide (Nylon).

Ø 20mm tube.

Concealed fixings.

30-year warranty.