**Lift-up shower seat with ALU leg- Large model**

Wall-mounted lift-up shower seat

White powder-coated aluminium structure

Reference: **510410**

Specification description

Lift-up ALU shower seat with leg.

Shower seat for disabled people and people with reduced mobility.

Lift-up: retained in upright position and slowed down descent.

Large model.

Large plastic slats, comfortable and easy to maintain.

Ergonomic non-slip side grips.

Folding leg guided by an articulated arm.

Structure made from white aluminium tube Ø 25mm x 2mm.

Concealed fixings.

Supplied with stainless steel screws for concrete walls.

Dimensions: 430 x 465 x 480mm.

Folded dimensions: 82 x 565mm.

Seat height: 480mm.

Leg height can be adjusted up to 8mm.

Tested to over 200kg. Maximum recommended user weight: 135kg.

Wall-mounted lift-up shower seat with 30-year warranty. CE marked.