**Stainless steel rectangular mirror, H. 500mm**

Unbreakable mirror

"Mirror" polished 304 stainless steel

Reference: **3452**

Specification description

Wall-mounted "mirror" polished bacteriostatic 304 stainless steel rectangular mirror.

Reinforced by a concealed solid PVC plate 10mm thick.

5 fixing points. Concealed fixings.

For installation on a flat surface.

Unbreakable mirror.

Dimensions: 10 x 385 x 485mm.

30-year warranty.